* Large Capacitor pad size/placement needs revision
* Change Connected and RX/TX LEDs to green
* Double check all resistor values
* BURN 560Ω resistors in HELL!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
* ~~Fix LED decal~~
* ~~Fix diode decal~~